Motion sensor light

(DH499)

Thank you for purchasing from RNIB. In the unlikely event the item is unsuitable, please contact us within 14 days of receipt to obtain your returns number. To ensure your return goes smoothly, the item and all components must be in as new condition and packed in its original, undamaged packaging. For further details and guidance on returning faulty items, please see the Terms and conditions of sale and How to contact RNIB sections of this instruction manual.

Please retain these instructions for future reference.

General description

This light provides a bright white beam (50–80 lumens) when it detects movement up to 3 metres away. It will only activate in low-light conditions to minimise battery usage and switches off 30 seconds after movement stops.

It is ideal for lighting dark cupboards, wardrobes, or drawers, or for providing low-level lighting in hallways or other dim areas.

The light swivels within its frame, allowing you to angle it towards the required area.

Powered by 3 × AA 1.5 V alkaline batteries (not supplied). It can be fixed to any flat, dry, indoor, or weather-protected surface using screws or the double-sided adhesive pad provided.

Orientation

The light measures approximately 259 × 26 × 22 mm (10.1 × 1.1 × 0.8 inches). It is a tubular plastic lamp mounted in a flat metal frame. On the front of the lamp, at one end, there is a square black button switch and a round, dome-shaped opaque movement sensor. On the back of the lamp, in the centre, is the battery compartment with a small semi-circular catch at one end.

Operation

To insert or replace the batteries, rotate the lamp tube while keeping the frame still so that the back of the lamp faces you. Locate the battery cover catch and gently pull it towards the centre while lifting to remove the cover. Insert the 3 × AA batteries one after the other with the positive terminal first. For the final battery, press it lightly against the spring (negative end) before lowering it into place. Replace the cover.

To switch the lamp on or off

Press the black square button on the front of the light. When the light comes on, the movement sensor is activated. The lamp will automatically switch off after 30 seconds and remain in automatic mode, turning on again whenever movement is detected. (Note: the sensor only operates in low light or darkness.) To switch the lamp off completely, press the black button again — this also disables the sensor.

Guarantee

This product is guaranteed against manufacturing faults for 12 months from the date of purchase. If you have any problems, please contact your retailer or supplier first. At the end of the product’s life, you may return it to the supplier or manufacturer for free disposal in accordance with the Waste Electrical and Electronic Equipment Directive.

Terms and conditions of sale

This product is guaranteed from manufacturing faults for 12 months from the date of purchase.

For all returns contact RNIB. You can request full terms and conditions from RNIB or view them online.

How to contact RNIB

Phone: 0303 123 9999

Email: shop@rnib.org.uk

Online Shop: shop.rnib.org.uk

 \*\*\*

Products are provided by RNIB Enterprises Limited. Company number: 0887094 Registered office: The Grimaldi Building, 154a Pentonville Road, London N1 9JE.  RNIB Enterprises Limited is a trading subsidiary of the Royal National Institute of Blind People, a charity registered in England and Wales (226227) and Scotland (SC039316).

Date: October 2025.