LED floor light with fan
(DH509)
Thank you for purchasing from RNIB. This item has been supplied by a third party. In the unlikely event the item is unsuitable, please contact us within 14 days of receipt to obtain your returns number. To ensure your return goes smoothly, the item and all components must be in as new condition and packed in its original, undamaged packaging. For further details and guidance on returning faulty items, please see the Terms and conditions of sale and How to contact RNIB sections of this instruction manual. 
 
Please retain these instructions for future reference. 
  
Thank you for purchasing this LED Floor Light with Fan which offers a cooling breeze while providing a good quality light.  This multi-height lamp features 3 different wind speeds and a choice of warm white, cool white or daylight colour temperatures. 	

Please take the time to read this document thoroughly to familiarise yourself with how the unit works and to ensure you get many years of safe use from this product.

Figure 1
Shows a remote control, with numbers 1 & 2 on the top, from left to right; numbers 3 & 4 just below, also from left to right; the 6 is just below 3 & 4 in the centre; a little below the 6 are two numbers 5 one on the left and one on the right; in the centre between the 5s is a setup button, and below this is a single 6 so that the two 6s are on the top and bottom of the central setup button; just below the right-hand 5 is a number 7 just slightly to the left. Near the bottom of the control are 3 fan shapes; under each one is 1, with an 8 under it; a 2, with an 8 under it; a 3, with an 8 under it, and a small fan ON and under this is a fan shape OFF, and a 9 under it.


1. Light On/Off
2. All Off
3. Colour temperature Choice	a) Fan On/Speed Select/Off
4. Night Light	                        b) Light On/Colour Select/Off
5. Colour Temperature Adjust	c) Increase Brightness (Hold)
6. Brightness Adjust	                d) Decrease Brightness (Hold)
7. Neutral Light (4000K)	        e) USB Power Socket
8. Fan Speed Select (1 - 3)
9. Fan On/Off

The a) to e) above are to be found on the stand of the fan. 

Figure 2. Assembly Instructions 
Your light is supplied in sections to aid transportation and requires basic assembly before use.  The unit is supplied with 3 sections of pole offering the option of 4 height levels.  Assembly should be completed with reference to FIGURE 2 as follows. 

For use as a desk light, the LIGHT HEAD (a) should be screwed directly into BASE (b), taking care not to cross-thread the screw connection.
For use as a floor light, screw together the desired number of EXTENSION POLES (c),  taking care not to cross-thread the screw connection.  Connect LIGHT HEAD (a) to the upper-most EXTENSION POLE (c) and the BASE (b) to the lower-most EXTENSION POLE (c). 

Operating Instructions 

Following assembly, place the unit on a firm, flat surface prior to connecting to a power source.  With reference to FIGURE 1, plug one end of the supplied USB C cable into the USB power socket (e) and the other end into a suitable mains USB adapter.  
 
Operating the Fan
The fan may be controlled using the touch control pad or the supplied remote. From the touch control pad, repeatedly press the FAN button (a) to turn the fan on, select each of the 3 speeds and, finally, turn the unit off.  
 
From the remote control, press the FAN button (9) to turn the fan on or off.  Press the relevant FAN SPEED button (8) to select correct speed.  The light and fan can be turned off by pressing the ALL OFF button (2).

Operating the Light
The light may be controlled using the touch control pad or the supplied remote. From the touch control pad, repeatedly press the LIGHT button (b) to turn the light on, select each of the colour temperatures in turn and, finally, turn the unit off.
 
From the remote control, press the LIGHT button (1) to turn the light on or off. Press the COLOUR TEMPERATURE buttons (3) or UP and DOWN buttons (6) to select each of the colour temperatures in turn. The light and fan can be turned off by pressing the ALL OFF button (2).
 
Brightness Adjustment
From the touch control pad, hold the PLUS button (c) to increase the brightness. To reduce the brightness, hold the MINUS button (d).
 
From the remote control, press the LEFT or RIGHT buttons (5) to change the brightness of the light. The remote control also offers two presets for colour temperature and brightness. The NIGHT LIGHT button (4) sets the light to a warm white light at a low brightness level. The 4000K button (7) sets the light to a bright, daylight temperature.
 
Maintenance, Cleaning and Safety Precautions
When not used for an extended period, your light should be unplugged and stored in a cool, dry location.
The light and fan may be cleaned with a soft, dry cloth. Avoid the use of cleaning products or solvents.
 
Warranty 
(Please visit www.lifemaxuk.co.uk/warranty to register)
In the unlikely event that your item develops a manufacturing fault, it is covered by a one year return to base warranty. Your warranty runs for 12 months from the date of purchase and is only valid with the original receipt, please ensure you keep this safe. Your warranty does not cover consumables, misuse or customer damage and will be deemed void where the repairs have been attempted by an unauthorised agent. This does not affect your statutory rights.
 
If your product develops a defect during the warranty period, please call the helpline number for further advice. If instructed, please securely pack your item and return enclosing your contact details, proof of purchase and fault details. We will, at our discretion, repair or exchange the item in line with warranty legislation. Where no proof of purchase is provided, or the product is outside the warranty period, repairs/replacements will be offered at cost to the customer.
 
Technical specification

	Product
	Size (Max.)
	H184xD28cm
	Weight
	3.9kg
	Material
	ABS + Iron

	Power
	Mains
	USB Type C
	Voltage
	DC 5V / 3A
	Maximum
	15W

	Light Source
	Type / Lifespan
	LED > 30,000hrs
	Tempera-ture
	3,000K - 6,500K
	Colour Rendering Index
	≥ 92




Terms and conditions of sale
This product is guaranteed from manufacturing faults for 12 months from the date of purchase.  
  
For all returns and repairs contact RNIB. You can request full terms and conditions from RNIB or view them online.   

How to contact RNIB  
Phone: 0303 123 9999  
Email: shop@rnib.org.uk  
Online Shop: shop.rnib.org.uk  
  
Products are provided by RNIB Enterprises Limited. Company number: 0887094 Registered office: The Grimaldi Building, 154a Pentonville Road, London N1 9JE. RNIB Enterprises Limited is a trading subsidiary of the Royal National Institute of Blind People, a charity registered in England and Wales (226227) and Scotland (SC039316). 

Date: July 2026.
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