Uno pro floor lamp (DH507)
Thank you for purchasing from RNIB. This item has been supplied by a third party. In the unlikely event the item is unsuitable, please contact us within 14 days of receipt to obtain your returns number. To ensure your return goes smoothly, the item and all components must be in as new condition and packed in its original, undamaged packaging. For further details and guidance on returning faulty items, please see the Terms and conditions of sale and How to contact RNIB sections of this instruction manual. 
 
Please retain these instructions for future reference. 
  
Daylight Guarantee/Warranty
This product is guaranteed against mechanical and electrical defects. For full Daylight guarantee Terms & Conditions please refer to the Daylight website. Faulty products should be returned to the place of purchase and proof of purchase must be presented. 
Please quote the model number in all correspondence. Returned products damaged by poor packaging are the responsibility of the sender. During the guarantee period, Daylight will repair or replace the product free of charge provided the fault was not caused by misuse, improper handling, negligence, normal wear and tear, accidental damage, or by any modifications made by the purchaser. The guarantee does not cover consumables such as bulbs, tubes or batteries. This guarantee does not affect your statutory rights.
This light source (LED only) is replaceable by manufacturer, by service personnel authorised by the manufacturer or by a comparably qualified person.
This product contains a light source (LED only) of energy efficiency class < D >
Getting started
1. Remove all packaging from around the lamp and place the base on the floor.
2. Feed the connector and cable (5) through the TOP pole (2) until the connector comes out of the end. 
(NOTE: The TOP Pole is WITHOUT the silver male thread at one end). Screw the Top pole (2) to the end of the flexible arm (1), taking care not to cross the threads. Tighten firmly.
3. Feed the connector & cable (5) through the SILVER THREAD of the BOTTOM Pole (3) until the connector comes out of the end. Screw the bottom pole (3) to the top pole (2), taking care not to cross the threads. Tighten firmly. 
4. Feed the connector & cable (5) through the hole in the floor base (4) and then screw the complete pole assembly onto the floor base, taking care not to cross the threads. Tighten firmly. 
5. Connect the power adapter jack to the connector on the cable and plug into a suitable electrical socket.
6. Switch the lamp on by touching the symbol at the end of the lamp shade. Subsequent touches of the symbol allows the 4 different brightness levels and OFF to be selected.
IMPORTANT SAFETY INSTRUCTIONS – PLEASE SAVE FOR FUTURE REFERENCE.
CAUTION: DO NOT LOOK DIRECTLY AT THE LEDS.
BEFORE CLEANING MAKE SURE THE LAMP IS DISCONNECTED FROM THE ELECTRICAL SUPPLY.
IN CASE OF DOUBT CONSULT A QUALIFIED ELECTRICIAN.
FOR INDOOR USE ONLY.
Thank you for purchasing this Daylight product. To read more information about your guarantee, please go to www.daylightcompany.com. To ensure correct and safe operation please read the following and retain for future reference.
If the lamp requires cleaning simply wipe with a damp cloth. Do not use large amounts of liquid or spray cleaners as they may enter the lamp and affect electrical safety.
CAUTION: DO NOT LOOK DIRECTLY AT THE LEDS.
CAUTION: If the cable of this luminaire becomes damaged, it should be exclusively replaced by a suitably qualified person in order to avoid hazard.
No maintenance is required. The LEDs are not user replaceable as they are designed to last for the lifetime of the product.
Terms and conditions of sale
This product is guaranteed from manufacturing faults for 24 months from the date of purchase.  
  
For all returns and repairs contact RNIB. You can request full terms and conditions from RNIB or view them online.   

How to contact RNIB  
Phone: 0303 123 9999  
Email: shop@rnib.org.uk  
Online Shop: shop.rnib.org.uk  
  
Products are provided by RNIB Enterprises Limited. Company number: 0887094 Registered office: The Grimaldi Building, 154a Pentonville Road, London N1 9JE.  RNIB Enterprises Limited is a trading subsidiary of the Royal National Institute of Blind People, a charity registered in England and Wales (226227) and Scotland (SC039316).

Date: June 2026.
1

