Wafer 1 A4 light pad (DH508)
Thank you for purchasing from RNIB. This item has been supplied by a third party. In the unlikely event the item is unsuitable, please contact us within 14 days of receipt to obtain your returns number. To ensure your return goes smoothly, the item and all components must be in as new condition and packed in its original, undamaged packaging. For further details and guidance on returning faulty items, please see the Terms and conditions of sale and How to contact RNIB sections of this instruction manual. 
 
Please retain these instructions for future reference. 
IMPORTANT SAFETY INSTRUCTIONS - PLEASE SAVE FOR FUTURE REFERENCE.
Thank you for purchasing this Daylight product. To read more information about your guarantee, please go to www.daylightcompany.com. To ensure correct and safe operation please read the following and retain for future reference.
Set-up and Operation
1. Before use remove all packaging from around the lightpad and place on a level surface.
2. Use the supplied USB cable to connect power to the lightpad. Insert the USB-C connector into the side of the lightpad and connect the USB-A connector to any 5V/2A (Maximum) USB power source (such as a plug-in adapter, USB power strip, laptop, or power bank). 
Important: Use Only the Supplied USB-A to USB-C Cable.
3. Switch on by touching the power symbol, touch again to change between the 3 brightness levels and to switch off.
4. When not in use disconnect from the USB power source.
Cleaning
BEFORE CLEANING MAKE SURE THE LIGHTPAD IS DISCONNECTED FROM THE ELECTRICAL SUPPLY.
If the lightpad requires cleaning simply wipe with a damp cloth. Do not use large amounts of liquid or spray cleaners as they may enter the lightpad and affect electrical safety.
Take particular care when cleaning the acrylic surface of the unit. To avoid scratches, use only a soft cotton cloth dampened with a little warm soapy water. NEVER USE AN ABRASIVE CLEANER.
Maintenance & Safety
No maintenance is required. The LEDs are not user or service replaceable as they are designed to last for the lifetime of the product.
FOR INDOOR USE ONLY.
Caution: 
If the cable of this luminaire becomes damaged, it should be exclusively replaced by a suitably qualified person in order to avoid hazard.
IN CASE OF DOUBT CONSULT A QUALIFIED ELECTRICIAN.

Terms and conditions of sale
This product is guaranteed from manufacturing faults for 24 months from the date of purchase.  
  
For all returns and repairs contact RNIB. You can request full terms and conditions from RNIB or view them online.   

How to contact RNIB  
Phone: 0303 123 9999  
Email: shop@rnib.org.uk  
Online Shop: shop.rnib.org.uk  
  
Products are provided by RNIB Enterprises Limited. Company number: 0887094 Registered office: The Grimaldi Building, 154a Pentonville Road, London N1 9JE.  RNIB Enterprises Limited is a trading subsidiary of the Royal National Institute of Blind People, a charity registered in England and Wales (226227) and Scotland (SC039316). 
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